<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 15:12:47</description>
<packages>
<package name="QFP80P900X900X160-33N">
</package>
<package name="QFN65P700X700X100-33N">
</package>
<package name="QFP50P900X900X160-48N">
</package>
<package name="QFN50P800X800X100-49N">
</package>
<package name="QFP50P1200X1200X160-64N">
</package>
<package name="QFN40P800X800X100-65N">
</package>
</packages>
<symbols>
<symbol name="VNC2-32L1B">
<pin name="VCCIO_3.3V" direction="pwr"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="VCCIO_3.3V_3" direction="pwr"/>
<pin name="1.8V_VCC_PLL_IN" direction="pwr"/>
<pin name="1.8V_VREG_OUT" direction="pwr"/>
<pin name="3.3V_VREG_IN" direction="pwr"/>
<pin name="XTIN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RESET"/>
<pin name="PROG" direction="in"/>
<pin name="USB1DP"/>
<pin name="USB1DM"/>
<pin name="USB2DP"/>
<pin name="USB2DM"/>
<pin name="GND_PLL" direction="pas"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_CORE_3" direction="pas"/>
<pin name="XTOUT" direction="out"/>
<pin name="IO_BUS0"/>
<pin name="IO_BUS1"/>
<pin name="IO_BUS2"/>
<pin name="IO_BUS3"/>
<pin name="IO_BUS4"/>
<pin name="IO_BUS5"/>
<pin name="IO_BUS6"/>
<pin name="IO_BUS7"/>
<pin name="IO_BUS8"/>
<pin name="IO_BUS9"/>
<pin name="IO_BUS10"/>
<pin name="IO_BUS11"/>
</symbol>
<symbol name="VNC2-32Q1B">
<pin name="VCCIO_3.3V" direction="pwr"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="VCCIO_3.3V_3" direction="pwr"/>
<pin name="1.8V_VCCPLL_IN" direction="pwr"/>
<pin name="3.3V_VREG_IN" direction="in"/>
<pin name="PROG" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_CORE_3" direction="pas"/>
<pin name="GNDPLL" direction="pas"/>
<pin name="EPAD" direction="in"/>
<pin name="XTOUT" direction="out"/>
<pin name="USB1DP"/>
<pin name="USB2DP"/>
<pin name="USB1DM"/>
<pin name="USB2DM"/>
<pin name="1.8V_VREG_OUT" direction="out"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
</symbol>
<symbol name="VNC2-48L1B">
<pin name="VCCIO_3.3V"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="VCCIO_3.3V_3" direction="pwr"/>
<pin name="VCCPLL_IN" direction="pwr"/>
<pin name="3.3V_VREG_IN" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="PROG" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="USB1DP"/>
<pin name="USB1DM"/>
<pin name="USB2DM"/>
<pin name="USB2DP"/>
<pin name="GNDPLL" direction="pas"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_CORE_3" direction="pas"/>
<pin name="XTOUT" direction="out"/>
<pin name="1.8V_VREG_OUT" direction="out"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
</symbol>
<symbol name="VNC2-48Q1B">
<pin name="VCCIO_3.3_V" direction="pwr"/>
<pin name="VCCIO_3.3V" direction="pwr"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="1.8_VCC_PLL_IN" direction="pwr"/>
<pin name="1.8_VREG_OUT" direction="pwr"/>
<pin name="3.3_VREG_IN" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="PROG" direction="in"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_PLL" direction="pas"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_CORE_3" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
<pin name="XTOUT" direction="out"/>
<pin name="USB1DP"/>
<pin name="USB1DM"/>
<pin name="USB2DP"/>
<pin name="USB2DM"/>
</symbol>
<symbol name="VNC2-64L1B">
<pin name="VCCIO_3.3V" direction="pwr"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="1.8V_VCCPLL_IN" direction="pwr"/>
<pin name="VCCIO_3.3VGND" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="PROG" direction="in"/>
<pin name="3.3V_VREG_IN" direction="in"/>
<pin name="XTIN" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="USB1DM"/>
<pin name="USB2DM"/>
<pin name="USB1DP"/>
<pin name="USB2DP"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_CORE_3" direction="out"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_PLL" direction="out"/>
<pin name="1.8V_VREGOUT" direction="out"/>
<pin name="XTOUT" direction="out"/>
<pin name="IOBUS0_2"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS0"/>
<pin name="IOBUS11"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
<pin name="IOBUS28"/>
<pin name="IOBUS29"/>
<pin name="IOBUS30"/>
<pin name="IOBUS31"/>
<pin name="IOBUS32"/>
<pin name="IOBUS33"/>
<pin name="IOBUS34"/>
<pin name="IOBUS35"/>
<pin name="IOBUS36"/>
<pin name="IOBUS37"/>
<pin name="IOBUS38"/>
<pin name="IOBUS39"/>
<pin name="IOBUS40"/>
<pin name="IOBUS41"/>
<pin name="IOBUS42"/>
<pin name="IOBUS43"/>
</symbol>
<symbol name="VNC2-64Q1B">
<pin name="VCCIO_3.3V" direction="pwr"/>
<pin name="VCCIO_3.3V_2" direction="pwr"/>
<pin name="VCCIO_3.3V_3" direction="pwr"/>
<pin name="3.3_VREG_IN" direction="pwr"/>
<pin name="1.8_VCC_PLL_IN" direction="pwr"/>
<pin name="1.8_VREG_OUT" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="PROG" direction="in"/>
<pin name="USB1DP"/>
<pin name="USB1DM"/>
<pin name="USB2DP"/>
<pin name="USB2DM"/>
<pin name="GND_CORE" direction="pas"/>
<pin name="GND_CORE_2" direction="pas"/>
<pin name="GND_CORE_3" direction="pas"/>
<pin name="GND_IO" direction="pas"/>
<pin name="GND_PLL" direction="pas"/>
<pin name="EPAD" direction="pas"/>
<pin name="XTOUT" direction="out"/>
<pin name="IOBUS0"/>
<pin name="IOBUS1"/>
<pin name="IOBUS2"/>
<pin name="IOBUS3"/>
<pin name="IOBUS4"/>
<pin name="IOBUS5"/>
<pin name="IOBUS6"/>
<pin name="IOBUS7"/>
<pin name="IOBUS8"/>
<pin name="IOBUS9"/>
<pin name="IOBUS10"/>
<pin name="IOBUS11"/>
<pin name="IOBUS12"/>
<pin name="IOBUS13"/>
<pin name="IOBUS14"/>
<pin name="IOBUS15"/>
<pin name="IOBUS16"/>
<pin name="IOBUS17"/>
<pin name="IOBUS18"/>
<pin name="IOBUS19"/>
<pin name="IOBUS20"/>
<pin name="IOBUS21"/>
<pin name="IOBUS22"/>
<pin name="IOBUS23"/>
<pin name="IOBUS24"/>
<pin name="IOBUS25"/>
<pin name="IOBUS26"/>
<pin name="IOBUS27"/>
<pin name="IOBUS28"/>
<pin name="IOBUS29"/>
<pin name="IOBUS30"/>
<pin name="IOBUS31"/>
<pin name="IOBUS32"/>
<pin name="IOBUS33"/>
<pin name="IOBUS34"/>
<pin name="IOBUS35"/>
<pin name="IOBUS36"/>
<pin name="IOBUS37"/>
<pin name="IOBUS38"/>
<pin name="IOBUS39"/>
<pin name="IOBUS40"/>
<pin name="IOBUS41"/>
<pin name="IOBUS42"/>
<pin name="IOBUS43"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VNC2-32L1B" prefix="U">
<description>Embedded Dual USB Host Controller</description>
<gates>
<gate name="A" symbol="VNC2-32L1B"/>
</gates>
<devices>
<device name="" package="QFP80P900X900X160-33N">
<connects>
<connect gate="A" pin="1.8V_VCC_PLL_IN" pad="3"/>
<connect gate="A" pin="1.8V_VREG_OUT" pad="7"/>
<connect gate="A" pin="3.3V_VREG_IN" pad="2"/>
<connect gate="A" pin="GND_CORE" pad="1"/>
<connect gate="A" pin="GND_CORE_2" pad="19"/>
<connect gate="A" pin="GND_CORE_3" pad="27"/>
<connect gate="A" pin="GND_IO" pad="16"/>
<connect gate="A" pin="GND_PLL" pad="6"/>
<connect gate="A" pin="IO_BUS0" pad="11"/>
<connect gate="A" pin="IO_BUS1" pad="12"/>
<connect gate="A" pin="IO_BUS10" pad="31"/>
<connect gate="A" pin="IO_BUS11" pad="32"/>
<connect gate="A" pin="IO_BUS2" pad="14"/>
<connect gate="A" pin="IO_BUS3" pad="15"/>
<connect gate="A" pin="IO_BUS4" pad="23"/>
<connect gate="A" pin="IO_BUS5" pad="24"/>
<connect gate="A" pin="IO_BUS6" pad="25"/>
<connect gate="A" pin="IO_BUS7" pad="26"/>
<connect gate="A" pin="IO_BUS8" pad="29"/>
<connect gate="A" pin="IO_BUS9" pad="30"/>
<connect gate="A" pin="PROG" pad="9"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="18"/>
<connect gate="A" pin="USB1DP" pad="17"/>
<connect gate="A" pin="USB2DM" pad="21"/>
<connect gate="A" pin="USB2DP" pad="20"/>
<connect gate="A" pin="VCCIO_3.3V" pad="28"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="13"/>
<connect gate="A" pin="VCCIO_3.3V_3" pad="22"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-32L1B"/>
<attribute name="OC_FARNELL" value="1863854"/>
<attribute name="OC_NEWARK" value="27T5918"/>
<attribute name="PACKAGE" value="QFP-32"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-32Q1B" prefix="U">
<description>Dual USB Host Controller IC</description>
<gates>
<gate name="A" symbol="VNC2-32Q1B"/>
</gates>
<devices>
<device name="" package="QFN65P700X700X100-33N">
<connects>
<connect gate="A" pin="1.8V_VCCPLL_IN" pad="3"/>
<connect gate="A" pin="1.8V_VREG_OUT" pad="7"/>
<connect gate="A" pin="3.3V_VREG_IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="33"/>
<connect gate="A" pin="GNDPLL" pad="6"/>
<connect gate="A" pin="GND_CORE" pad="27"/>
<connect gate="A" pin="GND_CORE_2" pad="1"/>
<connect gate="A" pin="GND_CORE_3" pad="19"/>
<connect gate="A" pin="GND_IO" pad="16"/>
<connect gate="A" pin="IOBUS0" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS10" pad="31"/>
<connect gate="A" pin="IOBUS11" pad="32"/>
<connect gate="A" pin="IOBUS2" pad="14"/>
<connect gate="A" pin="IOBUS3" pad="15"/>
<connect gate="A" pin="IOBUS4" pad="23"/>
<connect gate="A" pin="IOBUS5" pad="24"/>
<connect gate="A" pin="IOBUS6" pad="25"/>
<connect gate="A" pin="IOBUS7" pad="26"/>
<connect gate="A" pin="IOBUS8" pad="29"/>
<connect gate="A" pin="IOBUS9" pad="30"/>
<connect gate="A" pin="PROG" pad="9"/>
<connect gate="A" pin="RESET" pad="10"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="18"/>
<connect gate="A" pin="USB1DP" pad="17"/>
<connect gate="A" pin="USB2DM" pad="21"/>
<connect gate="A" pin="USB2DP" pad="20"/>
<connect gate="A" pin="VCCIO_3.3V" pad="13"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="22"/>
<connect gate="A" pin="VCCIO_3.3V_3" pad="28"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-32Q1B"/>
<attribute name="OC_FARNELL" value="1863855"/>
<attribute name="OC_NEWARK" value="27T5919"/>
<attribute name="PACKAGE" value="QFN-32"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-48L1B" prefix="U">
<description>Vinculum-II Embedded Dual USB Host Controller IC</description>
<gates>
<gate name="A" symbol="VNC2-48L1B"/>
</gates>
<devices>
<device name="" package="QFP50P900X900X160-48N">
<connects>
<connect gate="A" pin="1.8V_VREG_OUT" pad="7"/>
<connect gate="A" pin="3.3V_VREG_IN" pad="2"/>
<connect gate="A" pin="GNDPLL" pad="6"/>
<connect gate="A" pin="GND_CORE" pad="1"/>
<connect gate="A" pin="GND_CORE_2" pad="39"/>
<connect gate="A" pin="GND_CORE_3" pad="27"/>
<connect gate="A" pin="GND_IO" pad="24"/>
<connect gate="A" pin="IOBUS0" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS10" pad="22"/>
<connect gate="A" pin="IOBUS11" pad="23"/>
<connect gate="A" pin="IOBUS12" pad="31"/>
<connect gate="A" pin="IOBUS13" pad="32"/>
<connect gate="A" pin="IOBUS14" pad="33"/>
<connect gate="A" pin="IOBUS15" pad="34"/>
<connect gate="A" pin="IOBUS16" pad="35"/>
<connect gate="A" pin="IOBUS17" pad="36"/>
<connect gate="A" pin="IOBUS18" pad="37"/>
<connect gate="A" pin="IOBUS19" pad="38"/>
<connect gate="A" pin="IOBUS2" pad="13"/>
<connect gate="A" pin="IOBUS20" pad="41"/>
<connect gate="A" pin="IOBUS21" pad="42"/>
<connect gate="A" pin="IOBUS22" pad="43"/>
<connect gate="A" pin="IOBUS23" pad="44"/>
<connect gate="A" pin="IOBUS24" pad="45"/>
<connect gate="A" pin="IOBUS25" pad="46"/>
<connect gate="A" pin="IOBUS26" pad="47"/>
<connect gate="A" pin="IOBUS27" pad="48"/>
<connect gate="A" pin="IOBUS3" pad="14"/>
<connect gate="A" pin="IOBUS4" pad="15"/>
<connect gate="A" pin="IOBUS5" pad="16"/>
<connect gate="A" pin="IOBUS6" pad="18"/>
<connect gate="A" pin="IOBUS7" pad="19"/>
<connect gate="A" pin="IOBUS8" pad="20"/>
<connect gate="A" pin="IOBUS9" pad="21"/>
<connect gate="A" pin="PROG" pad="10"/>
<connect gate="A" pin="RESET" pad="9"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="26"/>
<connect gate="A" pin="USB1DP" pad="25"/>
<connect gate="A" pin="USB2DM" pad="29"/>
<connect gate="A" pin="USB2DP" pad="28"/>
<connect gate="A" pin="VCCIO_3.3V" pad="17"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="30"/>
<connect gate="A" pin="VCCIO_3.3V_3" pad="40"/>
<connect gate="A" pin="VCCPLL_IN" pad="3"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-48L1B"/>
<attribute name="OC_FARNELL" value="1863856"/>
<attribute name="OC_NEWARK" value="27T5920"/>
<attribute name="PACKAGE" value="LQFP-48"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-48Q1B" prefix="U">
<description>Embedded Dual USB Host Controller</description>
<gates>
<gate name="A" symbol="VNC2-48Q1B"/>
</gates>
<devices>
<device name="" package="QFN50P800X800X100-49N">
<connects>
<connect gate="A" pin="1.8_VCC_PLL_IN" pad="3"/>
<connect gate="A" pin="1.8_VREG_OUT" pad="7"/>
<connect gate="A" pin="3.3_VREG_IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="49"/>
<connect gate="A" pin="GND_CORE" pad="1"/>
<connect gate="A" pin="GND_CORE_2" pad="27"/>
<connect gate="A" pin="GND_CORE_3" pad="39"/>
<connect gate="A" pin="GND_IO" pad="24"/>
<connect gate="A" pin="GND_PLL" pad="6"/>
<connect gate="A" pin="IOBUS0" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS10" pad="22"/>
<connect gate="A" pin="IOBUS11" pad="23"/>
<connect gate="A" pin="IOBUS12" pad="31"/>
<connect gate="A" pin="IOBUS13" pad="32"/>
<connect gate="A" pin="IOBUS14" pad="33"/>
<connect gate="A" pin="IOBUS15" pad="34"/>
<connect gate="A" pin="IOBUS16" pad="35"/>
<connect gate="A" pin="IOBUS17" pad="36"/>
<connect gate="A" pin="IOBUS18" pad="37"/>
<connect gate="A" pin="IOBUS19" pad="38"/>
<connect gate="A" pin="IOBUS2" pad="13"/>
<connect gate="A" pin="IOBUS20" pad="41"/>
<connect gate="A" pin="IOBUS21" pad="42"/>
<connect gate="A" pin="IOBUS22" pad="43"/>
<connect gate="A" pin="IOBUS23" pad="44"/>
<connect gate="A" pin="IOBUS24" pad="45"/>
<connect gate="A" pin="IOBUS25" pad="46"/>
<connect gate="A" pin="IOBUS26" pad="47"/>
<connect gate="A" pin="IOBUS27" pad="48"/>
<connect gate="A" pin="IOBUS3" pad="14"/>
<connect gate="A" pin="IOBUS4" pad="15"/>
<connect gate="A" pin="IOBUS5" pad="16"/>
<connect gate="A" pin="IOBUS6" pad="18"/>
<connect gate="A" pin="IOBUS7" pad="19"/>
<connect gate="A" pin="IOBUS8" pad="20"/>
<connect gate="A" pin="IOBUS9" pad="21"/>
<connect gate="A" pin="PROG" pad="10"/>
<connect gate="A" pin="RESET" pad="9"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="26"/>
<connect gate="A" pin="USB1DP" pad="25"/>
<connect gate="A" pin="USB2DM" pad="29"/>
<connect gate="A" pin="USB2DP" pad="28"/>
<connect gate="A" pin="VCCIO_3.3V" pad="30"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="40"/>
<connect gate="A" pin="VCCIO_3.3_V" pad="17"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-48Q1B"/>
<attribute name="OC_FARNELL" value="1863857"/>
<attribute name="OC_NEWARK" value="27T5921"/>
<attribute name="PACKAGE" value="QFN-48"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-64L1B" prefix="U">
<description>Vinculum-II Embedded Dual USB Host Controller IC</description>
<gates>
<gate name="A" symbol="VNC2-64L1B"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X160-64N">
<connects>
<connect gate="A" pin="1.8V_VCCPLL_IN" pad="3"/>
<connect gate="A" pin="1.8V_VREGOUT" pad="7"/>
<connect gate="A" pin="3.3V_VREG_IN" pad="2"/>
<connect gate="A" pin="GND_CORE" pad="53"/>
<connect gate="A" pin="GND_CORE_2" pad="1"/>
<connect gate="A" pin="GND_CORE_3" pad="35"/>
<connect gate="A" pin="GND_IO" pad="30"/>
<connect gate="A" pin="GND_PLL" pad="6"/>
<connect gate="A" pin="IOBUS0" pad="22"/>
<connect gate="A" pin="IOBUS0_2" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS11" pad="23"/>
<connect gate="A" pin="IOBUS12" pad="24"/>
<connect gate="A" pin="IOBUS13" pad="25"/>
<connect gate="A" pin="IOBUS14" pad="26"/>
<connect gate="A" pin="IOBUS15" pad="27"/>
<connect gate="A" pin="IOBUS16" pad="28"/>
<connect gate="A" pin="IOBUS17" pad="29"/>
<connect gate="A" pin="IOBUS18" pad="31"/>
<connect gate="A" pin="IOBUS19" pad="32"/>
<connect gate="A" pin="IOBUS2" pad="13"/>
<connect gate="A" pin="IOBUS20" pad="39"/>
<connect gate="A" pin="IOBUS21" pad="40"/>
<connect gate="A" pin="IOBUS22" pad="41"/>
<connect gate="A" pin="IOBUS23" pad="42"/>
<connect gate="A" pin="IOBUS24" pad="43"/>
<connect gate="A" pin="IOBUS25" pad="44"/>
<connect gate="A" pin="IOBUS26" pad="45"/>
<connect gate="A" pin="IOBUS27" pad="46"/>
<connect gate="A" pin="IOBUS28" pad="47"/>
<connect gate="A" pin="IOBUS29" pad="48"/>
<connect gate="A" pin="IOBUS3" pad="14"/>
<connect gate="A" pin="IOBUS30" pad="49"/>
<connect gate="A" pin="IOBUS31" pad="50"/>
<connect gate="A" pin="IOBUS32" pad="51"/>
<connect gate="A" pin="IOBUS33" pad="52"/>
<connect gate="A" pin="IOBUS34" pad="55"/>
<connect gate="A" pin="IOBUS35" pad="56"/>
<connect gate="A" pin="IOBUS36" pad="57"/>
<connect gate="A" pin="IOBUS37" pad="58"/>
<connect gate="A" pin="IOBUS38" pad="59"/>
<connect gate="A" pin="IOBUS39" pad="60"/>
<connect gate="A" pin="IOBUS4" pad="15"/>
<connect gate="A" pin="IOBUS40" pad="61"/>
<connect gate="A" pin="IOBUS41" pad="62"/>
<connect gate="A" pin="IOBUS42" pad="63"/>
<connect gate="A" pin="IOBUS43" pad="64"/>
<connect gate="A" pin="IOBUS5" pad="16"/>
<connect gate="A" pin="IOBUS6" pad="17"/>
<connect gate="A" pin="IOBUS7" pad="18"/>
<connect gate="A" pin="IOBUS8" pad="19"/>
<connect gate="A" pin="IOBUS9" pad="20"/>
<connect gate="A" pin="PROG" pad="10"/>
<connect gate="A" pin="RESET" pad="9"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="34"/>
<connect gate="A" pin="USB1DP" pad="33"/>
<connect gate="A" pin="USB2DM" pad="37"/>
<connect gate="A" pin="USB2DP" pad="36"/>
<connect gate="A" pin="VCCIO_3.3V" pad="38"/>
<connect gate="A" pin="VCCIO_3.3VGND" pad="21"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="54"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-64L1B"/>
<attribute name="OC_FARNELL" value="1863858"/>
<attribute name="OC_NEWARK" value="27T5922"/>
<attribute name="PACKAGE" value="LQFP-64"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VNC2-64Q1B" prefix="U">
<description>Embedded Dual USB Host Controller</description>
<gates>
<gate name="A" symbol="VNC2-64Q1B"/>
</gates>
<devices>
<device name="" package="QFN40P800X800X100-65N">
<connects>
<connect gate="A" pin="1.8_VCC_PLL_IN" pad="3"/>
<connect gate="A" pin="1.8_VREG_OUT" pad="7"/>
<connect gate="A" pin="3.3_VREG_IN" pad="2"/>
<connect gate="A" pin="EPAD" pad="65"/>
<connect gate="A" pin="GND_CORE" pad="1"/>
<connect gate="A" pin="GND_CORE_2" pad="35"/>
<connect gate="A" pin="GND_CORE_3" pad="53"/>
<connect gate="A" pin="GND_IO" pad="30"/>
<connect gate="A" pin="GND_PLL" pad="6"/>
<connect gate="A" pin="IOBUS0" pad="11"/>
<connect gate="A" pin="IOBUS1" pad="12"/>
<connect gate="A" pin="IOBUS10" pad="22"/>
<connect gate="A" pin="IOBUS11" pad="23"/>
<connect gate="A" pin="IOBUS12" pad="24"/>
<connect gate="A" pin="IOBUS13" pad="25"/>
<connect gate="A" pin="IOBUS14" pad="26"/>
<connect gate="A" pin="IOBUS15" pad="27"/>
<connect gate="A" pin="IOBUS16" pad="28"/>
<connect gate="A" pin="IOBUS17" pad="29"/>
<connect gate="A" pin="IOBUS18" pad="31"/>
<connect gate="A" pin="IOBUS19" pad="32"/>
<connect gate="A" pin="IOBUS2" pad="13"/>
<connect gate="A" pin="IOBUS20" pad="39"/>
<connect gate="A" pin="IOBUS21" pad="40"/>
<connect gate="A" pin="IOBUS22" pad="41"/>
<connect gate="A" pin="IOBUS23" pad="42"/>
<connect gate="A" pin="IOBUS24" pad="43"/>
<connect gate="A" pin="IOBUS25" pad="44"/>
<connect gate="A" pin="IOBUS26" pad="45"/>
<connect gate="A" pin="IOBUS27" pad="46"/>
<connect gate="A" pin="IOBUS28" pad="47"/>
<connect gate="A" pin="IOBUS29" pad="48"/>
<connect gate="A" pin="IOBUS3" pad="14"/>
<connect gate="A" pin="IOBUS30" pad="49"/>
<connect gate="A" pin="IOBUS31" pad="50"/>
<connect gate="A" pin="IOBUS32" pad="51"/>
<connect gate="A" pin="IOBUS33" pad="52"/>
<connect gate="A" pin="IOBUS34" pad="55"/>
<connect gate="A" pin="IOBUS35" pad="56"/>
<connect gate="A" pin="IOBUS36" pad="57"/>
<connect gate="A" pin="IOBUS37" pad="58"/>
<connect gate="A" pin="IOBUS38" pad="59"/>
<connect gate="A" pin="IOBUS39" pad="60"/>
<connect gate="A" pin="IOBUS4" pad="15"/>
<connect gate="A" pin="IOBUS40" pad="61"/>
<connect gate="A" pin="IOBUS41" pad="62"/>
<connect gate="A" pin="IOBUS42" pad="63"/>
<connect gate="A" pin="IOBUS43" pad="64"/>
<connect gate="A" pin="IOBUS5" pad="16"/>
<connect gate="A" pin="IOBUS6" pad="17"/>
<connect gate="A" pin="IOBUS7" pad="18"/>
<connect gate="A" pin="IOBUS8" pad="19"/>
<connect gate="A" pin="IOBUS9" pad="20"/>
<connect gate="A" pin="PROG" pad="10"/>
<connect gate="A" pin="RESET" pad="9"/>
<connect gate="A" pin="TEST" pad="8"/>
<connect gate="A" pin="USB1DM" pad="34"/>
<connect gate="A" pin="USB1DP" pad="33"/>
<connect gate="A" pin="USB2DM" pad="37"/>
<connect gate="A" pin="USB2DP" pad="36"/>
<connect gate="A" pin="VCCIO_3.3V" pad="38"/>
<connect gate="A" pin="VCCIO_3.3V_2" pad="21"/>
<connect gate="A" pin="VCCIO_3.3V_3" pad="54"/>
<connect gate="A" pin="XTIN" pad="4"/>
<connect gate="A" pin="XTOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="VNC2-64Q1B"/>
<attribute name="OC_FARNELL" value="1863859"/>
<attribute name="OC_NEWARK" value="27T5923"/>
<attribute name="PACKAGE" value="QFN-64"/>
<attribute name="SUPPLIER" value="FTDI"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
