<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="STK6722_STANDART_UP">
</package>
</packages>
<symbols>
<symbol name="STK6722H">
<pin name="+VCC1"/>
<pin name="STM_1-1"/>
<pin name="VZ"/>
<pin name="STM_1-2"/>
<pin name="A"/>
<pin name="A*"/>
<pin name="STM_1-3"/>
<pin name="VCC2_SR"/>
<pin name="+VCC2"/>
<pin name="GND"/>
<pin name="PWM_OUT"/>
<pin name="STM_2-2"/>
<pin name="B"/>
<pin name="B*"/>
<pin name="STM_2-3"/>
<pin name="STM_2-1"/>
<pin name="PWM_CTR"/>
<pin name="OFF"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="STK6722H" uservalue="yes">
<description>Stepping motor driver wthis PWM</description>
<gates>
<gate name="G$2" symbol="STK6722H"/>
</gates>
<devices>
<device name="" package="STK6722_STANDART_UP">
<connects>
<connect gate="G$2" pin="+VCC1" pad="1"/>
<connect gate="G$2" pin="+VCC2" pad="9"/>
<connect gate="G$2" pin="A" pad="5"/>
<connect gate="G$2" pin="A*" pad="6"/>
<connect gate="G$2" pin="B" pad="13"/>
<connect gate="G$2" pin="B*" pad="14"/>
<connect gate="G$2" pin="GND" pad="10"/>
<connect gate="G$2" pin="OFF" pad="18"/>
<connect gate="G$2" pin="PWM_CTR" pad="17"/>
<connect gate="G$2" pin="PWM_OUT" pad="11"/>
<connect gate="G$2" pin="STM_1-1" pad="2"/>
<connect gate="G$2" pin="STM_1-2" pad="4"/>
<connect gate="G$2" pin="STM_1-3" pad="7"/>
<connect gate="G$2" pin="STM_2-1" pad="16"/>
<connect gate="G$2" pin="STM_2-2" pad="12"/>
<connect gate="G$2" pin="STM_2-3" pad="15"/>
<connect gate="G$2" pin="VCC2_SR" pad="8"/>
<connect gate="G$2" pin="VZ" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
